Back to Contents Page

# Specifications: Intel(R) PRO/Wireless 2200BG User's Guide

Specifications |

Form Factor | Mini PCI Type 3B
Dimensions | Width 2.34 in x Length 1.75 in x Height 0.20 in (59.45 mm x 44.45 mm x 5 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin SO-DIMM edge connector
Operating Temperature | 0 to +70 degrees Celsius
Humidity | 50 to 85% non-condensing

Type |

Frequency band | 2.400 - 2.472 GHz (US) 2.400 - 2.4835 GHz (Japan) 2.400 - 2.4835 GHz (Europe ETSI)

Frequency Modulation |

Modulation | OFDM with BPSK, QPSK, 16QAM, 64QAM, DBPSK, DQPSK, CCK
Channels | Full 14 channel support
Data Rates | 1, 2, 5.5, 6, 9, 11, 12, 24, 36, 48 and 54 Mbps
Indoor Range | 100 ft (30 m) @ 11 Mbps / 300 ft (90 m) @ 1 Mbps
Outdoor Range | 400 ft (120 m) @ 11 Mbps / 1500 ft (460 m) @ 1 Mbps

Power

Transmit Output Power | 16 dBm (typical)
Adapter Power Consumption
Transmit | 1.45 W
Receive | 0.85 W
Idle | 60 mw
Disable | 50 mw
Voltage | 3.3 V

General

Operating Systems | Windows* XP, 2000
Wi-Fi Alliance certification | Wi-Fi® certification for 802.11b and 802.11g
WLAN Standard | IEEE 802.11g
Architecture | Infrastructure or ad hoc (peer-to-peer)
Security | WPA, Cisco CCX v1.0, LEAP, PEAP, TKIP, EAP-TLS, EAP-TTLS, WEP 128-bit and 64-bit.
Product Safety | UL, C-UL, CB (IEC 60590)

Back to Contents Page

Please read all restrictions and disclaimers.